**ROMcard2 and NVMEcard DOS 3.3 patch:**

The pre-loaded DOS 3.3 in the “Patched” files is modified such that the 512kB memory also can contain 3

disk images (DSK) each starting at $03000, $26000 and $49000 respectively. The disk imaged can contain

files that use DOS to load, i.e., cannot be auto start disks.

The & command work for the individual files if written per original configuration.

The 3 disks are called by accessing them on the slot number as appropriate (S7 for slot 7) and the disk number 1,2 and 3, for instance:

CATALOG S7, D1

CATALOG S7, D2

CATALOG S7, D3